| API For Arduino developers

- Main Page
- Related Pages
- Classes
- Files
- Examples

- Class List
- Class Index
- Class Members

ESP8266 Member List

This is the complete list of members for ESP8266, including all inherited members.

createTCP(String addr, uint32_t port) | ESP8266 |
createTCP(uint8_t mux_id, String addr, uint32_t port) | ESP8266 |
deepSleep(uint32_t time) | ESP8266 |
disableMUX(void) | ESP8266 |
enableMUX(void) | ESP8266 |
getAPIp(uint8_t pattern=3) | ESP8266 |
getAPList(void) | ESP8266 |
getDHCP(uint8_t pattern=3) | ESP8266 |
getIPStatus(void) | ESP8266 |
getJoinedDeviceIP(void) | ESP8266 |
getLocalIP(void) | ESP8266 |
getNowConecAp(uint8_t pattern=3) | ESP8266 |
getSoftAPParam(uint8_t pattern=3) | ESP8266 |
getStationIp(uint8_t pattern=3) | ESP8266 |
getStationMac(uint8_t pattern=3) | ESP8266 |
getVersion(void) | ESP8266 |
getWifiModeList(void) | ESP8266 |
joinAP(String ssid, String pwd, uint8_t pattern=3) | ESP8266 |
kick(void) | ESP8266 |
leaveAP(void) | ESP8266 |
recv(uint8_t *buffer, uint32_t buffer_size, uint32_t timeout=1000) | ESP8266 |
recv(uint8_t mux_id, uint8_t *buffer, uint32_t buffer_size, uint32_t timeout=1000) | ESP8266 |
recv(uint8_t *coming_mux_id, uint8_t *buffer, uint32_t buffer_size, uint32_t timeout=1000) | ESP8266 |
registerUDP(String addr, uint32_t port) | ESP8266 |
registerUDP(uint8_t mux_id, String addr, uint32_t port) | ESP8266 |
releaseTCP(void) | ESP8266 |
releaseTCP(uint8_t mux_id) | ESP8266 |
restart(void) | ESP8266 |
restore(void) | ESP8266 |
saveTransLink(uint8_t mode, String ip, uint32_t port) | ESP8266 |
send(const uint8_t *buffer, uint32_t len) | ESP8266 |
send(uint8_t mux_id, const uint8_t *buffer, uint32_t len) | ESP8266 |
setAPIp(String ip, uint8_t pattern=3) | ESP8266 |
setAutoConnect(uint8_t en) | ESP8266 |
setCIPMODE(uint8_t mode) | ESP8266 |
setDHCP(uint8_t mode, uint8_t en, uint8_t pattern=3) | ESP8266 |
setEcho(uint8_t mode) | ESP8266 |
setOprToSoftAP(uint8_t pattern1=3, uint8_t pattern2=3) | ESP8266 |
setOprToStation(uint8_t pattern1=3, uint8_t pattern2=3) | ESP8266 |
setOprToStationSoftAP(uint8_t pattern1=3, uint8_t pattern2=3) | ESP8266 |
setPing(String ip) | ESP8266 |
setSoftAPParam(String ssid, String pwd, uint8_t chl=7, uint8_t ecn=4, uint8_t pattern=3) | ESP8266 |
setStationIp(String ip, String gateway, String netmask, uint8_t pattern=3) | ESP8266 |
setStationMac(String mac, uint8_t pattern=3) | ESP8266 |
setTCPServerTimeout(uint32_t timeout=180) | ESP8266 |
setUart(uint32_t baudrate, uint8_t pattern) | ESP8266 |
startServer(uint32_t port=333) | ESP8266 |
startSmartConfig(uint8_t type) | ESP8266 |
startTCPServer(uint32_t port=333) | ESP8266 |
stopServer(void) | ESP8266 |
stopSmartConfig(void) | ESP8266 |
stopTCPServer(void) | ESP8266 |
unregisterUDP(void) | ESP8266 |
unregisterUDP(uint8_t mux_id) | ESP8266 |