This is a library for the SHT31 Digital Humidity + Temp sensor

Designed specifically to work with the SHT31 Digital in the Adafruit shop 
  ----> https://www.adafruit.com/products/2857

These sensors use I2C to communicate, 2 pins are required to interface

Adafruit invests time and resources providing this open source code, 
please support Adafruit and open-source hardware by purchasing 
products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.  
BSD license, all text above must be included in any redistribution

Check out the links above for our tutorials and wiring diagrams 

To download. click the ZIP button in the top-middle navbar, 
rename the uncompressed folder Adafruit_SHT31. 
Check that the Adafruit_SHT31 folder contains Adafruit_SHT31.cpp and Adafruit_SHT31.h

Place the Adafruit_SHT31 library folder your arduinosketchfolder/libraries/ folder. 
You may need to create the libraries subfolder if its your first library. Restart the IDE.

We also have a great tutorial on Arduino library installation at:
http://learn.adafruit.com/adafruit-all-about-arduino-libraries-install-use